{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Foglio1","Foglio2","Foglio3"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Foglio1","index":0,"n_rows":19,"n_cols":13,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
{"$rows_empty":8}
[null,null,null,"Come l'ho ricavata vedi immagine "]
[]
[]
[]
[{"$nulls":6},"Inserire il ",null,"Valore di L cercata  "]
[null,null,"Ro",null,"MHz ",null,"Ros voluto ",null,"micro Henry  ",null,"tau ",null,"dB"]
[null,null,"ohm ",null,"Frequenza minima ",{"$nulls":5},"coef, Riflessione ",null,"attenuaz.di rilessione "]
[null,null,50,null,50,null,1.05,null,3.2633601165476396,null,0.02439024390243905,null,-32.2556771343947]
[null,null,50,null,50,null,1.1,null,1.670077783710431,null,0.04761904761904766,null,-26.444385894678376]
[null,null,50,null,7,null,1.05,null,23.309715118197424,null,0.02439024390243905,null,-32.2556771343947]
[null,null,73,null,50,null,2,null,0.328782133927503,null,0.3333333333333333,null,-9.542425094393248]

{"sheet":"Foglio2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Foglio3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}